Acoustic Positioning Workflow –set up, import, position receivers at depth, then position tags

1. Project Setup
2. Temperature Assessment
3. Metronome – limit to receivers at surface
4. Clock Fix Serial – fix only those receivers that we know positions of
5. Multipath – beacon tags of receivers at depth
6. Coordinate With Deng – individual tags (receivers at depth)
   1. When complete - add coordinates to master tag table – median of all positions
7. Metronome – limit to receivers at depth
8. Clock Fix Serial – limit to receivers at depth
9. Multipath – All study tags
10. Send to Tom for positioning